Hydro

horizontal distance between sound source and hydrophone, m depth of the sound source, m

TDOA,sec between direct signal and Echo from bottom for all source locations

2000 1714 1429 1143 857 571 286 0

500

1000

1500

2000

2500 0

0.05

0.1

0.15

0.2

0.25

0.3

0.35

0.4

0.45

0.5